Type I Permit- $54.00

1. Bonfires
2. The use of a torch or flame producing device to remove paint from, or seal membrane roofs on any building or structure
3. The occasional use of any non residential occupancy other than Use Groups F, H or S for group overnight stays of persons over 2 ½ years of age, in accordance with section F-709.0 of the Fire Prevention Code
4. Individual portable kiosks or displays when erected in covered mall for a period of less than 90 days and when not covered by a Type 2 permit
5. The use of any open flame or flame producing device in connection with any public gathering for purposes of entertainment, amusement or recreation
6. Welding and cutting operations except where the welding and cutting is performed in areas approved for welding and is registered as a type B Life Hazard use
7. The possession or use of explosives or blasting agents, other than model rocketry engines regulated under NJAC 12:194
8. The use of any open flame or flame producing device in connection with the training of non-fire service personnel in fire suppression or extinguishment procedures
9. The occasional use in any building of a multipurpose room with a maximum permitted occupancy of 100 or more for amusement, entertainment or mercantile type purposes
10. The storage or handling of class I flammable liquids in closed containers of aggregate amounts of more than 10 gallons, but not more than 660 gallons inside a building or more than 60 gallons but not more than 66o gallons outside a building.
11. The storage of handling of class II or IIIA combustible liquids in closed containers of aggregate amounts of more than 25 gallons but not more than 660 gallons inside a building or more than 60 gallons, but not more than 660 gallons outside a building.
12. Any permanent cooking operation that requires a suppression system in accordance with NJAC 5:70-4(g) and is not defined as a life hazard use in accordance with NJAC 5:70-2.4
13. The use as a place of public assembly for a total of not more than 15 days in a calendar year of building classified as a commercial farm building under the Uniform Construction Code.

Type 2 Permit – 214.00

1. Bowling lane resurfacing and bowling pin refinishing involving the use and application of flammable liquids or materials
2. Fumigation or thermal insecticide fogging
3. Carnivals and circuses employing mobile structure used for human occupancy
4. The use of a covered mall in any of the following manners
   1. Placing or constructing temporary kiosks, display booths, concession equipment or the lide in more than 25 percent of the common area of the mall
   2. Temporarily using the mall as a place of assembly
   3. Using open flame devices
   4. Displaying liquid or gas fueled power equipment or
   5. Using liquefied petroleum gas, liquefied natural gas and compressed flammable gas in containers exceeding 5 pound capacity
5. Storage outside of building of LP-gas cylinders when part of a cylinder exchange program